Activity 1:

1. 0x00400000 for text segment, 0x10010000 for Data segment
2. Basic we can only see the hex values/addresses are shown with numbers
3. 32 bytes
4. 8 columns
5. The relation is each column represents at 4 bytes
6. Line 3
7. 0x10010000
8. Line 4/ascii/2 bytes for each ascii
9. 10010004
10. yes
11. la $a0, str 1

syscall

1. la == load the address

Activity 2:

1. done
2. li $v0, 5

syscall

1. li $v0, 5
2. done
3. done
4. done
5. done
6. done